REC 8.6 Tools in EasyC Name:

OBJECTIVE:

In this section, you will be introduced to the following tools in easyC:  
 **http://10.53.55.104/file.php/11/moddata/udutu/101/course/bullet.gifController Configurationhttp://10.53.55.104/file.php/11/moddata/udutu/101/course/blank.gif  
http://10.53.55.104/file.php/11/moddata/udutu/101/course/bullet.gifPort Descriptionshttp://10.53.55.104/file.php/11/moddata/udutu/101/course/blank.gif  
http://10.53.55.104/file.php/11/moddata/udutu/101/course/bullet.gifThe On-Line Window**

**Questions:**

1. The \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_allows you to directly control each motor port in real-time from easyC.
2. The [**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**](javascript:switchImage(%22UDUTU_MultiMedia1%22,%22Image%22,%22../media/content/rec02_controller_config_411142_520x390.jpg%22,%220%22,390,520)) allows you to label ports on the robot.
3. What does the the Controller Configuration Window allow you to do?
4. The Controller Configuration Window also allows you to label \_\_\_\_\_\_\_\_\_\_ and \_\_\_\_\_\_\_ ports.
5. What must be download on the controller in order for the On-Line Window to work properly?
6. The On-Line Window can be accessed by selecting [**\_\_\_\_\_\_\_\_\_\_\_\_\_**](javascript:switchImage(%22UDUTU_MultiMedia1%22,%22Image%22,%22../media/content/rec02_tools_ow_411150_520x390.jpg%22,%220%22,390,520)) or by clicking the icon on the Menu Bar.
7. How do you enter a port description in the On-Line Window ?
8. What are the two windows where you can change the description of a sensor?